UVI Dial-In Network Access� With Windows


Charles Balch, 1995 version 1.0


Many persons will want to take advantage of our dial-in access to run programs that traditionally run on networked computers.  This document shows how.


�
Requirements


A computer running Windows.


A modem, properly connected.


An account on GECKO.  Call John Lucas at 693-1216 for an account.


WINSOCK.DLL


TWINSOCK.EXE, FTP from FTP.UVI.EDU or see me.


Desired software such as:


NETSCAPE.EXE	Internet Navigator


EUDORA.EXE	Electronic Mail


WT_WSK.EXE	News Reader


WS_FTP.EXE	FTP 


Finding and installing these applications is beyond the scope of this handout.  Call me.


Instillation


� EMBED PBrush  ���


Put the UVI Install Dial-In Access disk into your disk drive.  Switch to that drive and type Install.


Start Twinsock by double clicking its icon. 


Under Communications in the Setup menu, configure Twinsock with the following.


Port	Probably COM1 or COM2


Speed	Your modem’s maximum speed up to 9600


Data bits	8


Parity	None


Stop Bits	1


Test your connection by typing ATA from within Twinsock and listening for a dial tone.  If you don’t hear a dial tone try a different COM port.  Then slower speeds. (The maximum speed on UVI modems is 9600).


�Usual Instructions


Note that the above software and our phone lines are not perfect.  You may have to repeat the following instructions a few times before you make it “in.”  Once you’re in you may hang-up or being disconnected.  From my personal experience, I would grade the system as good.  I find it works best to connect, get all my mail, disconnect, compose my replies and connect again.  This is also the most polite procedure since it leaves the port open for others.  


Be sure to disconnect when finished!


Connecting


Start Twinsock.


Under the Setup menu choose Dial and call UVI at 693-1570. Don’t forget to add 9 if on campus (or don’t use the 693).  I’m told that putting “*70,” in front of your number turns off Call Waiting but it hasn’t worked for me. 


After a while you will see Connect 9600 (or whatever speed your modem is set at).


Press the Enter key a few times and you should be prompted with a UVI-NET> prompt.


At the UVI-NET> prompt type GECKO then enter..


When prompted, log in by typing your account name, pressing enter, then typing your password (your password will not be displayed on the screen).


After a short message, a prompt with your account name (i.e. cbalch@gecko>) will appear.  


At the prompt, type tshost.  The Twinsock application should “disappear” (actually it is minimizing itself).


You can now run any of the applications mentioned above.


Disconnecting


Press ALT-TAB until you see Twinsock.


Select Disconnect from the Setup menu


Type EXIT at your prompt


Free your phone line unplugging it for a few seconds or by typing +++ then ATH after you are prompted by OK.


